**Tinbum Tuning**

**Bespoke Airgun Parts**

**Drop-in Kit Contents -** 1 x Spring Guide (long), 1 x Top Hat (short), 1 x Slip Washer (10mm hole), 2 x Power Washers (15mm hole), abrasive paper and Moly grease

**Assemble plastic parts in the piston without the spring prior to fitting.**

**If the rear guide isn’t sitting flush on the piston skirt the gun wont cock**

**and the guide needs to be shortened. Also check the guides fit to the**

**spring. In the unlikely event that it doesn’t fit, simply return the kit**

**along with your spring for an FOC bespoke replacement.**

TbT kits are designed to be used in place of factory power washers, spring guides

and top hats where fitted. Check carefully for weights and washers in the front of

the piston, especially HW models !

The slip washer is installed into the piston first, if you have made a sleeve the slip

washer will hold it in place. Use a small amount of a suitable airgun grease on the

piston rod and the machined face of the washer. The top hat goes in next with a

small amount of grease where it is in contact with the spring. After putting the

(lightly greased) spring in, put a smear of grease on the shaft of the spring guide

and insert into the spring.

Reassemble the gun and check the power. The supplied power washers can be

used on the rear of the spring guide to increase power if required.

**Tinbum Tuning accept no responsibility for your rifles legality**. After any work

check power levels with a chrono!

Technical support :

Email : support@airrifletuning.com

www.airrifletuning.com

Tel : 07545 147 459